**Chit Resolution Report for TF/OH Bundle Repair**

**NSTXU\_1-1-3-3-1\_CRR\_101, Rev 1 (Also includes SBS 1.1.3.3.2)**

Antonio Falcon Digitally Date: 2020.03.05 signed by 14:19:13 Antonio -05'00'

Falcon

Prepared By: A. Falcon, Cognizant Individual

Yuhu Zhai Digitally signed by Yuhu Zhai

Date: 2020.03.06 13:22:28 -05'00' Approved By: Y, Zhai, NSTX-U Project Engineer

Robert Ellis

Digitally Date: -05'00'

2020.03.06 signed by 14:47:25

Robert Ellis

Approved By: R. Ellis, Chief Engineer

**Record of Changes**

**Rev. Date Description of Changes**

0 1/31/2020 Initial Release 1 2/17/2020 Added Post FDR CHITs

**Summary of Chits**

**Review ID Status**

Magnets DVVR MTF04 Closed

Magnets DVVR MTF06 Closed

Magnets DVVR MTF13 Closed

Magnets DVVR MTF22 Closed

Magnets DVVR MTF30 Closed

Magnets DVVR MTF34 Closed

Magnets DVVR MTF36 Closed

Magnets DVVR MTF39 Closed

Magnets DVVR MOH03 Closed

Magnets DVVR MOH05 Closed

Magnets DVVR TFOH02 Closed

Magnets DVVR TFOH03 Closed

TF/OH Bundle Reliability

PDR TFOHBUNRELPDR01 Closed

TF/OH Bundle Reliability

PDR TFOHBUNRELPDR02 Closed

TF/OH Bundle Reliability

PDR TFOHBUNRELPDR03 Closed

TF/OH Bundle Reliability

PDR TFOHBUNRELPDR04 Closed

TF/OH Bundle Reliability

PDR TFOHBUNRELPDR05 Closed

TF/OH Bundle Reliability

PDR TFOHBUNRELPDR06 Closed

TF/OH Bundle Reliability

PDR TFOHBUNRELPDR07 Closed

Page 3 of 9

TF/OH Bundle Reliability

PDR TFOHBUNRELPDR08 Closed

Magnets DVVR MTF30 Closed

Cooling Water System

Interlock PDR CWSINTPDR01 Closed Cooling Water System

Interlock PDR CWSINTPDR02 Closed Cooling Water System

Interlock PDR CWSINTPDR03 Closed Cooling Water System

Interlock PDR CWSINTPDR04 Closed Cooling Water System

Interlock PDR CWSINTPDR05 Closed Cooling Water System

Interlock PDR CWSINTPDR06 Closed Cooling Water System

Interlock PDR CWSINTPDR07 Closed Cooling Water System

Interlock PDR CWSINTPDR08 Closed Cooling Water System

Interlock PDR CWSINTPDR09 Closed Cooling Water System

Interlock PDR CWSINTPDR10 Closed Cooling Water System

Interlock PDR CWSINTPDR11 Closed Cooling Water System

Interlock PDR CWSINTPDR12 Closed

Magnet RP Scope FDR 1 RPMAGTASK1-01 Closed

Magnet RP Scope FDR 1 RPMAGTASK1-02 Closed

Magnet RP Scope FDR 1 RPMAGTASK1-03 Closed

Magnet RP Scope FDR 1 RPMAGTASK1-04 Closed

Magnet RP Scope FDR 2 RPMAGTASK2-01 Closed

Magnet RP Scope FDR 2 RPMAGTASK2-02 Closed

Page 4 of 9

Magnet RP Scope FDR 2 RPMAGTASK2-03 Closed

Magnet RP Scope FDR 2 RPMAGTASK2-04 Closed

Magnet RP Scope FDR 3 PRMAGSCOPEFDRIII01 Closed

Magnet RP Scope FDR 3 PRMAGSCOPEFDRIII02 Closed

Magnet RP Scope FDR 3 PRMAGSCOPEFDRIII03 Closed

Magnet RP Scope FDR 3 PRMAGSCOPEFDRIII04 Closed

Magnet RP Scope FDR 3 PRMAGSCOPEFDRIII05 Closed

Page 5 of 9

**Table of Contents**

1 FDR CHITS 7 2 Cooling Fitting Upgrade 9 3 TFOL Cooling Tubes 9 4 Cap Block Rings 10 5 OH Ground Plane 11 6 OH Ground Plane Strap 11 7 TF/OH Grounding 12 8 Ground Plane Resistivity 12 9 Ground Plane Power Dissipation 12 10 Aquapour 13 11 OH Shims 13 12 Humidity 14 13 Parker and Swagelok 14 14 Megger/Hipot 14 15 Preload Bolt Tension 15 16 Cooling Water Interlock 15

Page 6 of 9

**1 FDR CHITs**

**Review ID Chit**

Magnet RP Scope FDR 1 RPMAGTASK1-01

Consider issuing a drawing ECN to the TF Bundle water fitting drawing to resolve the parker/swagelock disparity in lieu of a visual inspection (which requires kapton removal). Closed: Concur, a note will be added to the new TF Bundle drawing noting parker/swagelock fittings are nearly identical. No need to do visual inspection for part

**Review ID Chit**

Magnet RP Scope FDR 3 PRMAGSCOPEFD

RIII02

NSTXU\_1-1-3-3-2\_CALC\_100 is pending review in DMS. However, the signatories on DMS don't match those on the PDF uploaded to the FDR II dashboard. Furthermore, the draft uploaded in DMS is altogether missing the calc and checker forms which appear in the PDF. Please ensure that the DMS upload includes all pages (calc & checking) and has the appropriate signatories. Please ensure that it then gets fully signed in DMS.

Magnet RP Scope FDR 3

NSTXU-CALC-133-20-00 is a legacy calculation but the link in the NSTXU Documents Index is broken. Calculation is not retrievable. Please work with Kathleen to ensure that, at a minimum, the link PRMAGSCOPEFD

is restored (pending a mass migration of legacy documents into RIII03

DMS).

Magnet RP Scope FDR 1 RPMAGTASK1-04

NSTXU\_1-1-3-3-2\_CALC\_100 has been properly signed via PDF signatures. There is a pending DMS entry for it, but the review/approval personnel that were defined in DMS don't match those that signed the PDF. Work with Kathleen to ensure consistency when this CALC gets uploaded to DMS. Closed: CALC properly uploaded and approved in DMS on 2/28/2020

**Review ID Chit**

Magnet RP Scope FDR 2 RPMAGTASK2-01

Please review your resolution to chit \*PDR09 and PDR12...can't use budget justifications for these. Explain how Yuhu's calculation and the existing instrumentation configuration show the machine is properly protected.

For Yuhu's calculation and 09, I believe the answer is that the allowed tolerance on flow is generous, and so small variations in flow are not important.

For 12, the P&ID 5GA522 needs to be examined to resolve the issue. Closed: Readdressed the previous CHITs PDR09 and PDR12. PDR09: NSTXU\_1-1- 3\_CALC\_101 shows that the flow tolerance is great, and small variations are inconsequential PDR12: Drawing 5GA522 Sheet 19 details PF5 instrumented with two supply valves and one return, which accommodates for either supply

Page 7 of 9

**Review ID Chit**

Magnet RP Scope FDR 2 RPMAGTASK2-04

The posted DRP is not numbered and not signed. DRP needs to be properly finalized in DMS. Since this is a different scope from FDR1, please ensure you don't overwrite the FDR1 DRP. Need an DRP for each, I suppose, since they're separate scopes. Magnet RP Scope FDR 3 PRMAGSCOPEFDR

III04

The DRP posted on the dashboard requires the document # and rev fields populated on the front page. It must then be uploaded and fully signed in DMS.

Magnet RP Scope FDR 1 RPMAGTASK1-02

The Design Review Plan needs to be finalized & signed (if available, consider populating the CRR number and including CALC\_100. Closed: DRP signed 2/25

**Review ID Chit**

Magnet RP Scope FDR 2 RPMAGTASK2-03

I am concerned that the strategy that has been developed, while correct for plasma/coil operations, is not correct for the bakeout configuration. This is a requirements problem first, then an issue with design (but is luckily only a SW issue). Please work with Gerhardt/Cropper/Petrella to sort this out. Closed: Auxillary Requirements document has been updated with the proper language to capture the full design. The DC supplies have flow switches that are read by the Bakeout PLC, and Cooling provisions for the TF coil shall be identical to that during normal operations.

Page 8 of 9

**Review ID Chit**

Magnet RP Scope FDR 3

PRMAGSCOPEFD RIII01

NSTXU\_1-1-3-3-1\_CRR\_101 must be fully signed and posted in DMS

Magnet RP Scope FDR 2 RPMAGTASK2-02

CRR has been signed in PDF, but is called CRR\_XXX. Please obtain a valid DMS number and file in DMS. Thank you.

Magnet RP Scope FDR 1 RPMAGTASK1-03

Chits from previous review need to be officially closed. This means we need to finalize (sign/file) the Chit Resolution Report. Closed: Uploaded to DMS on 2/27/2020

**Review ID Chit**

Magnet RP Scope FDR 3

PRMAGSCOPEFD RIII05

Please make a measurement of the resistivity of the "grout" material. Closed: Resistivity will be measured and noted in report

**2 Cooling Fitting Upgrade**

**Review ID Chit**

Magnets DVVR

MTF04 Perform the cooling fitting upgrade/retrofit to the fittings in the

upper bulkhead

Magnets

DVVR MTF34

Lack of hardware verification during the assembly of coil cooling systems

Closed: CHIT RPMAGTASK1-01 Rejects these CHITs as unnecessary as Swagelok and Parker have nearly identical specs. Testing will still be done on the fittings following ENG-014

**3 TFOL Cooling Tubes**

**Review ID Chit**

Magnets DVVR MTF06 The cooling tubes on the new TFOL were damaged during

manufacturing. They were repaired, but it is unclear that they are reliable enough to last the full NSTX-U shot cycle

Page 9 of 9

Cooling tubes on several of the inner legs were twisted/distorted

Magnets DVVR MTF13

during removal from VPI mold. They passed all pressure and flow tests and have been strain relieved, however care must be taken when working neat or with thses components

Magnets DVVR MTF36

The TF water tubes extend top and bottom and are vulnerable to damage. While care is used in handling, some small dings and detentes appear. These tubes are difficult to mend, require protection if possible, and need delicate care during maintenance evolutions to avoid water leaks and thus preserve the life of the Centerstack.

Closed: -Hydrostatic tests were performed after after fabrication to 1.5x operating levels. We will perform this test again

-Hydrostatic tests are performed again after re-assembly of connecting hoses to 1.5x operating levels.

-Tubes are physically protected in-place by barriers.

-Tubes are inaccessible from outside the machine once assembled.

**4 Cap Block Rings**

**Review ID Chit**

Magnets DVVR MTF22

Examine the spacing and material of the Cap Block rings (top and bottom) and cooling tubes. "Top Cap Block Ring" and "Bulk Head Block Inner Ring

Closed: No Stainless Steel materials located near energized parts. No action needed other than to update the drawing.

**5 G-10 plate**

**Review ID Chit**

Magnets

DVVR MTF39 Thermal stresses between thick G-10 plate and cooling tubes at the

top/bottom of TF cool.

Closed: Cooling tube thermal expansion accommodated by nitrile washer between bulkhead bracket and G-10 bulkhead. Also addressed by simple hand calculation at a separate review by Steve R. explaining the G10 washers provide more than adequate relief for thermal growth

Page 10 of 9

**6 OH Ground Plane**

**Review ID Chit**

Magnets

DVVR MOH03 Resistivity of the OH ground plane does not meet original

requirement. Re-apply to proper specification

Closed: Perform OH Ground Plane Test Procedure to apply paint and measure the resistivity to ensure limits are within range.

**7 OH Ground Plane Strap**

**Review ID Chit**

Magnets

DVVR MH05

Consider re-design of OH ground plane strap to eliminate reliance on a single break, and improve attachment scheme. Introduce a second break, or otherwise reduce chance of toroReviewal short. Reduce reliance on G-10 piece to hold in place, if G-10 breaks then strap will fall off. TF/OH Bundle Reliability PDR

Confirm adequacy of upper ground plane electrical connection (the intent of the chit MOH5)

Closed: MH05: A review of supporting calculations indicate the forces on the plate are small. The G-10 used is used as an electrical isolation spacer, and not a mounting bracket. The existing design is simple and robust and does not require change.

Calculation NSTXU\_1\_1\_3\_3\_2\_CALC\_100\_OH\_Ground\_Plane has been filed and satisfies this CHIT

TFOHBUNRELPD R04

Page 11 of 9

**8 TF/OH Grounding**

**Review ID Chit**

Magnets

DVVR TFOH02

The wires in the TF-OH gap were grounded for the first run campaign. Recent calculations show that the electric field can be reduced by floating the wires. This should be assessed in light of larger grounding consideration.

Closed: The wires will be isolated from centerstack structural materials and brought to a termination block that is serviceable from the exterior of the machine. This will allow for floating, grounding, the addition of resistors, and the ability to test each wire in-situ.

**9 Ground Plane Resistivity**

**Review ID Chit**

TF/OH Bundle Reliability PDR

Please assess the documentation of the ground plane resistivity; calculation should be filed at minimum.

Closed: Calculation NSTXU\_1\_1\_3\_3\_2\_CALC\_100\_OH\_Ground\_Plane has been filed to detail ground plane resistivity requirements.

**10 Ground Plane Power Dissipation**

**Review ID Chit**

TF/OH Bundle Reliability PDR

TFOHBUNREL PDR02

Confirm that minimum tolerance value of ground plane paint TFOHBUNRELP

resistivity does not lead to excessive power/energy dissipation in the DR03

paint

Page 12 of 9

Closed: The voltage on the ground plane decays rapidly, from 600V to 50V in less than 30 milliseconds; therefore, the power dissipation is not a concern. See NSTXU\_1\_1\_3\_3\_2\_CALC\_100\_OH\_Ground\_Plane

**11 Aquapour**

**Review ID Chit**

Magnets DVVR

TFOH03 Wire stuck in Aquapour should be left floating, rather than tied to CS casing. This will minimize E-field perturbation and avoid bringing 2kV into the gap during CHI. Ends of wire should be insulated but accessible for periodic insulation resistance measurement

Closed: Same as TFOH02. The wires will be isolated from centerstack structural materials and brought to a termination block that is serviceable from the exterior of the machine. This will allow for floating, grounding, the addition of resistors, and the ability to test each wire in-situ.

**12 OH Shims**

**Review ID Chit**

TF/OH Bundle Reliability PDR

While this chit is out-of-scope for this PDR, the inspection of Aquapour wires evidenced as-built shims placed in-between the OH coil and its base. It is unclear if this as-built condition is a concern. It is recommended that the analysis group investigates whether motion between the OH and TF could cause issue with the visible interference with these shims and/or if the uneven bearing that the shims impose on the OH is problem.

TFOHBUNRELP DR01

TFOHBUNRELP DR01

Closed: This issue has been addressed in the G10 ring peer review and detailed calculation has been filed (NSTXU\_1-1-3-3\_CALC\_104. Additional prototype testing was conducted, and a grout filler will be added to distribute the loads more uniformly.

**Review ID Chit**

MCS LOWER G10 RING RESOLUT ION Peer

MCSLOW10RRES PR02

Consider if a “belly band” solution for keeping the shims in place will increase the risk of tracking across the tops of the TF Flags and take appropriate measures to minimize

Consider if a “belly band” solution for keeping the shims in place will increase the risk of tracking across the tops of the TF Flags and take appropriate measures to minimize

Page 13 of 9

Review

Closed: Installation Procedure will be utilized to cover the TF faces, flash-shield slots, and any areas the epoxy may contaminate

**13 Humidity**

**Review ID Chit**

TF/OH Bundle Reliability PDR

The NTC humidity and therefore dew point is a significant risk to the machine beyond the Facilities responsibility to proves it. Evaluate dew point control requirements, define interfaces for hardware, responsibilities, and operations, revise operating procedures, ensure adequacy of interlocks, and considers RAMI.

Closed: The facilities are updating the HVAC system to address the cooling and particularly the humidity/dew point. The requirements of ~35% dew point have been included in the facilities scope for the test cell. In the mean-time, humidity and dew point remain a factor in conducting daily hi-pot tests.

**14 Parker and Swagelok**

**Review ID Chit**

TF/OH Bundle Reliability PDR

TFOHBUNRELPD R05

The Parker and Swagelok are each designed for ~4000psig. The as- built configuration (Parker nut/Swagelok body) should be pressure tested on bench to verify adequate margin.

Closed: All fittings will be tested according to ENG-014 Hydrostatic Test

**15 Megger/Hipot**

**Review ID Chit**

TF/OH Bundle Reliability PDR

TFOHBUNRELPD R07

Do a megger/hipot before FDR, but have an HV SME involved in the TFOHBUNRELPD

procedure and execution in order to assess the unusual R08

configuration.

Closed: A Megger Test schedule has been established. Every 6 months the test will be performed. Data is recorded and logged.

Page 14 of 9

**16 Preload Bolt Tension**

**Review ID Chit**

Magnets

DVVR MTF30

It sounded as a concern that if the preload bolts tension between the G-10 ring and SS flange is reduced, there is a concern that the slippage and twisting may develop at the flange-G10 interface. Install some positive means, like shear keys to prevent it and reduce the risk of motion

Closed: The preload tension on the bolts is significantly less that the allowable to the tension. Jiarong’s calculation shows loads of 600-1000 lbf.

1. Grout the Type-1 bolts to register the skirt interfaces to provide positive restraints at the

skirt interfaces. 2. Rely on the aquapour & friction, to provide restraint at the G10/TF interface.

**17 Cooling Water Interlock**

**Review ID Chit**

Cooling Water System Interlock PDR

The PLC software should annunciate which flow switch caused the system to trip - so we know which FS or flow path was the cause. Consider displaying this at PLC HMI and EPICS.

Closed: There are currently individual flow switch alarms that will be displayed at the local PLC HMI

**Review ID Chit**

Cooling Water System Interlock PDR

CWSINTPDR01

Revise the existing requirements document to specify if loss of flow in ANY cooling path shall shut the supply pumps down OR if only loss of flow on the TF & OH shall shut the supply pumps down. It is our CWSINTPDR02

current interpretation that any loss of flow event should shut the supply pumps down to minimize water leaks & potential damage from them, however the requirement document does not explicitly include paths other that the TF & OH.

Closed: Add the requirements to 3.1 c of Auxiliary Requirement Document

Page 15 of 9

When loss of flow is detected on any TF, OH, PF, or other misc. switch monitored by the cooling system, the supply pumps shall be shut down, and supply/return valves shall be turned off **Review ID Chit**

Cooling Water System Interlock PDR

The delamination risk exists for the TF outer legs as well; if cooling is lost in one of the conductors of the outer legs, but the others are cooled, then thermal stresses to some extent will develop. The requirements should reflect this case, either by stating the specific case of the outer TF legs, or a more generic statement about "loss of cooling" cases in coils with "bonded conductors".

Closed: By shutting the pumps and valves off to stop the water flowing, Yuhu has done a calc on the inner legs calc ref NSTXU\_1-1-3\_CALC\_101

**Review ID Chit**

Cooling Water System Interlock PDR

CWSINTPDR03

Add a mode to the logic to allow testing of flow switches during the morning startup (prior to plasma operations and excluding plasma operations) without dropping pumps out.

Closed: A test mode will be introduced to allow water to flow, and manually check each of the flow switches to ensure PLC reads correctly

**Review ID Chit**

Cooling Water System Interlock PDR

CWSINTPDR04

CWSINTPDR05 Is the resolution of the flow switches good enough to protect against

flow imbalances that would harm the coil.

Closed: By shutting the pumps and valves off when a leak is detected by the flow switch, we will reduce the flow imbalance that will keep harm to the coil at the minimum

Page 16 of 9

**Review ID Chit**

Cooling Water System Interlock PDR

CWSINTPDR06 Consider adding PLC logic to stop pumps based on differential

between water temperature of parallel cooling paths.

Closed: Considered, but not needed, because proposed change will shut down pumps and supply/return valves when an issue with the cooling path is detected.

**Review ID Chit**

Cooling Water System Interlock PDR

Need "bakeout" mode in Water System PLC to allow condition with flow in outer layer only during bakeout (desirable) without turning off pumps.

Closed: There is no bakeout flow switch detection path for the Cooling Water System. The bakeout PLC monitors the flow level

**Review ID Chit**

Cooling Water System Interlock PDR

CWSINTPDR07

CWSINTPDR08 Loss of flow triggers loss of permission for the next shot. Consider

interrupting the current shot & de-energizing magnets ASAP.

Closed: The loss of water will disable the permission for FCPC to arm the coil for the next shot. If a shot is started it will not be stopped.

**Review ID Chit**

Page 17 of 9

A discussion about detecting a partially blocked flowpath, a blockage that is insufficient to trip the flowswitch , could be detected by looking at the temperatures. This is a secondary detection of the

Cooling

flowrate.

Water System Interlock

There has been talk of installing flowmeters. If that work is done that would be a more direct method for detecting flow problems.

PDR

Consider deferring the analysis and programming to detect partial blockages until nearing coil-cooling operations, and if flowmeters have been installed a cost savings will be realized.

There is no requirement for partial flow.

Closed: NSTXU\_1-1-3\_CALC\_101 shows that the flow tolerance is great, and small variations are inconsequential

**Review ID Chit**

Cooling Water System Interlock PDR

CWSINTPDR09

For the FDR, will need to consider the new Software QA guidelines, if they are released. This may mean an independent code review of the ladder logic, or, software module testing if possible.

Closed: We are using the current approved Software Change Notice which follows the QA guidelines to update the software change.

**Review ID Chit**

Cooling Water System Interlock PDR

CWSINTPDR10

TF ONLY is a mode of the OH preheater system. In this mode OH water is valved off. This mode should be accommodated in the CWSINTPDR11

flowswitch-checking logic.

This nuance is not in the requirements for this review.

Closed: This will be part of the program change. During TF ONLY mode, only TF water flow switches are monitored

**Review ID Chit**

Page 18 of 9

Cooling Water System Interlock PDR

Consider adding individual flow switches in PF5Ua, PF5Ub, PF5La, CWSINTPDR012

PF5Lb, so that flow in individual a/b sub-coils can be detected and interlocked.

Closed: Drawing 5GA522 Sheet 19 details PF5 instrumented with two supply valves and one return, which accommodates for either supply

Page 19 of 9